Preserve Connector’s raw event on ArcMC

· These steps to enable preserve raw events on ArcMC WebUI.
· This document applies to both software and appliance ArcMC, on-board connectors as well remote-connectors.
1. Go to Node Management 
Select the connector by click to blank space next to the connector name.
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2. Select Runtime Parameters 
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3. Select the destination where you want to receive connector raw events
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4. Modify the destination settings
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5. Select Processing option to enable raw event
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6. Select “Yes” for Preserve Raw Event
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7. Confirm the changes 
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Notes:
The connector may need to restart, run for at least 10 mins to make sure we capture all connector raw events on destination.
Then we disable the Preserve Raw Event with the same steps as above.
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This process allows you to change the runtime parameters of connector destination(s). The wizard guides you
through the following steps:

- Selecting the destination(s) for the chosen connectors.
- Selecting the configuration(s) you wish to change.

- Selecting the parameter group.

- Entering the parameter values.
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